Aliases OwsDrv project of REXYGEN
=======================================

The source files in this folder form a project for the example of OwsDrv external configuration. This is the bare minimum 
to start the development from.

The executive of the project contains one task, which should be filled with 
function blocks to achieve the desired functionality.

## Timing of the project ##

The algorithm runs each 100 milliseconds (0.1 s). See the EXEC function block,  
tick x ntick0 = 0.05 x 2 = 0.1 

## Prerequisities ##
- *REXYGEN Runtime Core* must be installed and running on the target device.

## Running the example ##
- The **exec.mdl* file is the project main file.
- Open it with *REXYGEN Studio*.
- Drag&drop function blocks from the block library. 
- Compile and download the project to the target device.
- Switch to Watch mode and observe the algorithm in real-time.

## Documentation ##

- **Press F1 for help** on the selected function block in the *REXYGEN Studio*.
- [Function blocks of REXYGEN](https://www.rexygen.com/doc/PDF/ENGLISH/BRef_ENG.pdf)
- [REXYGEN Studio User Guide](https://www.rexygen.com/doc/PDF/ENGLISH/RexygenStudio_ENG.pdf)
- [Complete documentation of REXYGEN](http://www.rexygen.com/documentation-and-support)

## Additional information ##

- Visit the [REXYGEN webpage](http://www.rexygen.com) 
for more information about the example projects and developing advanced 
automation and control solutions using REXYGEN.